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Installation Manual

                                                                                                                     Ⅰ、Usage tool：                                                 
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spirit level 
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Ⅱ、Spare parts list：
1. Bottom orbit 1，    2. Handle 2，               3. Wall profile 2，

4. Vertical profile 2，          5. Fixed glass 2，           6. Upper rollers 4，                 

7. Wall plug 6，           8. Upper orbit 1，            9. Bottom bounce rollers 4，     

10. Magnetic plastic 2，     11. M4×35 Stud-Screw 8/M5×35Stud-Screw 6，
12. Waterproof 4，           13. M4×12 stud –screw 6，    14. Sealant 2，              
15. Moving glass 2,          16. The integral whole sealant 4
[image: image9.wmf]Ⅲ、Please check the quantity and quality of square parts before install, if you have any inquiry about it please contact our company or dealer without any hesitate, you will get satisfied reply soon!      
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1.  Please put the wall profile near the wall(Please 

install it according to the size of glass door),

and adjust the profile perpendicularly by spirit
level. Then drill by 6-8mm driller and put the 

wall plug into wall.
2. Putting the waterproof in side of fixed glass, insert

into the bottom and upper orbits and screw down the 

[image: image15.wmf]vertical profile by M4x30 screw(same as another            picture 2

side). Then drill in both of profiles by 3.2 driller. 

Screw down the decorating cover(picture 3) by 

M4x12 screw and insert the sealant into vertical 
profiles by small wood board(please make the
surface smooth).

3. Installing the upper and bottom rollers on the 
moving glass doors( two glass doors should be same),
then insert the waterproof plastic and magnetic
plastic on the side glass doosr and install the

handle. Put the moving glass doors into orbits,

Pressing the bottom rollers slightly, adjust          
the height of upper rollers by wrench until the
            picture 3
glass could work well.

4.  After the installation, all side of glass door should be silicone
5.  Please clear the frame by neutral purification after 8 hours.                          

Ⅵ、Please push the door slightly, don’t scratch the frame by strong and sharp material to avoid damaging fittings.
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