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Installation Manua
Ⅰ、Usage tool：                                                 
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driller        pencil         wrench 
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spirit level 
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Ⅱ、Spare parts list：
1.  base tray 1pcs    2. glass clip 2pcs，   3. wall profile 2pcs，    4. big glass (01) 1pcs，   5. Bracket 2set      6. Wall fastening for bracket 1pcs        7. Bracket clip  3pcs          8. corner profile  1pcs      9. big glass (02) 1pcs     10.small glass  1pcs             11. M5×35 screw 7pcs     12. M4×20 screw 2pcs              13. Wall plug 7pcs，      14. Sealant  4pcs,                  

Ⅲ、Please check the quantity and quality of the square parts before installation, if you have any inquiry about it, please contact our company or dealer without any hesitate, you will get satisfied reply soon！       
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Ⅴ、Installation process

1． [image: image10.wmf][image: image11.wmf]Please put the base tray in the floor and adjust it in balance by lever ruler, then put the wall profiles against the wall, measure the size on the wall and draw the hole according to the uprightness line, then drill by ф6mm driller and put the wall plug into wall. Screw down the wall profiles with the M5*30 screw.[image: image12.wmf]
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               Picture 1                                     Picture 2
2．Insert the big glass (01 ) and big glass (02) into the wall profile, pull them until the end, then stuff up them by the sealant.

3. Install the corner profile in the big glass (02), as picture 4, then insert the small glass to the  corner profile, as picture 5. finally insert a sealant to stuff up the glass. 
[image: image14.wmf]4. Put the whole set of brackets with wall fastening and bracket clip in the top of the glass in balance after assembling it , then put the wall fastening to the wall and line the position in the wall. as picture 6 & 7.
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Picture 3                   picture 4               Picture 5                picture 6
5. Put the wall fastening in the position we line on process 3, then drill by the ф6mm driller, insert the wall plug, then screw down the wall fastening to the wall by M5*30. As picture 8. 
6．Insert the brackets to the connector and nip with the two big glass by the glass clips, screw down it by the screw M4*20 after adjust.
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Picture 8                                           picture 9
7．After the installation, all side of glass door should be silicone.

8. Please clear the frame by neutral purification after 24 hours
Ⅵ. Please push the door slightly,don’t scratch the frame by strong and sharp material to avoid 
damaging fittings.  
� EMBED AutoCAD.Drawing.16 \* MERGEFORMAT ���





� EMBED AutoCAD.Drawing.16 \* MERGEFORMAT ���





� EMBED AutoCAD.Drawing.16  ���





� EMBED AutoCAD.Drawing.16 \* MERGEFORMAT ���





� EMBED AutoCAD.Drawing.16 \* MERGEFORMAT ���





� EMBED AutoCAD.Drawing.16 \* MERGEFORMAT ���





� EMBED AutoCAD.Drawing.16 \* MERGEFORMAT ���





� EMBED AutoCAD.Drawing.16 \* MERGEFORMAT ���





� EMBED AutoCAD.Drawing.16  ���











[image: image18.wmf][image: image19.wmf][image: image20.wmf]835

1435

[image: image21.wmf]3

4

1

2

5

6

7

8

9

10

[image: image22.wmf][image: image23.wmf]_1234567899.dwg

_1392202784.dwg

_1392202904.dwg

_1392203068.dwg

_1392203069.dwg

_1392203067.dwg

_1392202805.dwg

_1392202735.dwg

_1189928849.dwg

_1190630014.dwg

_1190630034.dwg

_1189942625.dwg

_1189928162.dwg

_1189928206.dwg

_1189927924.dwg

