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Installation Manual
Ⅰ、Usage tool：                                                 
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driller        pencil         wrench 
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   tape measure     hammer
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spirit level 
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Ⅱ、Spare parts list：
1. base tray 1pcs    2. glass clip 2pcs，   3. wall profile 2pcs，    4. big glass (01) 1pcs，   5. bracket 2set      6. wall fastening1pcs                7. bracket clip 3pcs          8. corner profile  1pcs      9. big glass (02) 1pcs     10.small glass  1pcs             11. M5×35 screw 7pcs     12. M4×20 screw 2pcs                13. Wall plug 7pcs，      14. Sealant  4pcs,                  

[image: image9.wmf]Ⅲ、Please check the quantity and quality of the square parts before installation, if you have any inquiry about it, please contact our company or dealer without any hesitate, you will get satisfied reply soon！       

Ⅴ、Installation process

1． [image: image10.wmf]Please put the base tray in the floor and adjust it in balance by lever ruler, then put the wall profiles against the wall, measure the size on the wall and draw the hole according to the uprightness line, then drill by ф6mm driller and put the wall plug into wall. Screw down the wall frame with the M5*30 screw.[image: image11.wmf]
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               Picture 1                                     Picture 2
2．Insert the big glass (01 ) and big glass (02) to the wall profiles, pull them until the end, then stuff up the them by the sealant.

3. Install the corner profile in the big glass (02), as picture 4, then insert the small glass to the corner profile, as picture 5. finally insert a sealant to stuff up the glass. 
4. Put the whole set of bracket in the top of the glass in balance after assembling it , then put the wall fastening to the wall and line the position in the wall. as picture 6 & 7.
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Picture 3                   picture 4               Picture 5                picture 6
5. Put the wall fastening in the position we line on process 3, then drill by the ф6mm driller, insert the wall plug, then screw down the wall fastening to the wall by M5*30. As picture 8. 
6．Insert the bracket to the connector and nip with the two big glass by the glass clips, screw down it by the screw M4*20 after adjust.
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Picture 8                                           picture 9
7．After the installation, all side of glass door should be silicone.

8. Please clear the frame by neutral purification after 24 hours
Ⅵ. Please push the door slightly,don’t scratch the frame by strong and sharp material to avoid 
damaging fittings.  
� EMBED AutoCAD.Drawing.16 \* MERGEFORMAT ���





� EMBED AutoCAD.Drawing.16 \* MERGEFORMAT ���





� EMBED AutoCAD.Drawing.16  ���





� EMBED AutoCAD.Drawing.16 \* MERGEFORMAT ���





� EMBED AutoCAD.Drawing.16 \* MERGEFORMAT ���





� EMBED AutoCAD.Drawing.16 \* MERGEFORMAT ���





� EMBED AutoCAD.Drawing.16 \* MERGEFORMAT ���





� EMBED AutoCAD.Drawing.16 \* MERGEFORMAT ���





� EMBED AutoCAD.Drawing.16  ���











[image: image18.wmf][image: image19.wmf][image: image20.wmf][image: image21.wmf]3

4

1

2

5

6

7

8

9

10

[image: image22.wmf][image: image23.wmf]_1234567899.dwg

_1392201235.dwg

_1392202382.dwg

_1392202689.dwg

_1392202690.dwg

_1392202509.dwg

_1392201240.dwg

_1392201074.dwg

_1189928849.dwg

_1190630014.dwg

_1190630034.dwg

_1189942625.dwg

_1189928162.dwg

_1189928206.dwg

_1189927924.dwg

