[image: image1.wmf]STAR  SHOWER ENCLOSURE

Installation Manual

                                                                                                                     Ⅰ、Usage tool：                                                 
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spirit level 
[image: image4.wmf]       screwdriver  
[image: image5.wmf]      small wood block 
[image: image6.wmf]   

Ⅱ、Spare parts list：
1. Wall profile 2,              2.Magnetic plastic 2,       3.Fixed glass 2,   

4. Sealant 2,       5.Wall plug 8,      6.Bracket 2,       7.Moving glass(door) 1,
8. Hinge 2,       9.Waterproof 1,     10. ST5×35 Stud-Screw 8/ ST4X20 Stud-Screw 2,
11. Bottom sealant waterproof 1,      12.Handle1,     13.defense water piece 2  
14. Profile waterproof in base 1
Ⅲ、Please check the quantity and quality of square parts before install, if you have any inquiry about it please contact our company or dealer without any hesitate, you will get satisfied reply soon!   
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picture 1
[image: image10.wmf]Ⅴ、Installation process：
[image: image11.wmf][image: image12.wmf]1. Please measure the size on the wall and draw the hole according to the uprightness line, then drill by ф6-8mm driller and put the wall plugs into wall. At last screw down the frame by M5x30 stud screw.

     picture 2                                              picture 3
2. Please insert the glass door into the wall profiles, and install the waterproof tightly, then screw down the brackets by M5*30 screw between top glass and wall. Insert the glass clip into the gap on the glass door, finally screw down by wrench.

3. Fixing the hinges on the fixed glass, and then link the moving glass door with hinges.
4. Again magnetic stripe waterproof a card is on the glass.             

5. After the installation, the wall side glass door should be silicone.

6. Please clear the frame by neutral purification after 8 hours.

Ⅵ、Please push the door slightly,don’t scratch the frame by strong and sharp material to avoid 
damaging fittings.
[image: image13.wmf]
picture 4
� EMBED AutoCAD.Drawing.16 \* MERGEFORMAT ���





� EMBED AutoCAD.Drawing.16 \* MERGEFORMAT ���





� EMBED AutoCAD.Drawing.16 \* MERGEFORMAT ���





� EMBED AutoCAD.Drawing.16 \* MERGEFORMAT ���





� EMBED AutoCAD.Drawing.16 \* MERGEFORMAT ���





� EMBED AutoCAD.Drawing.16 \* MERGEFORMAT ���








[image: image14.wmf][image: image15.wmf][image: image16.wmf]1

2

3

4

6

7

8

9

10

11

5

12

13

14

[image: image17.wmf]_1234567895.dwg

_1234567897.dwg

_1311665477.dwg

_1311666203.dwg

_1311665650.dwg

_1273491109.dwg

_1234567896.dwg

_1234567893.dwg

_1234567894.dwg

_1234567891.dwg

_1234567892.dwg

_1234567890.dwg

