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Ⅰ、Usage tool：                                                  
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Ⅱ、Spare parts list：
1.Handle 1 set (2pc),    2. M5×30 Stud-screw 6/ M4×35 Stud-screw 8,    3.Wall plugs 6,  

4.Fixed glass 2,         5.M4×12Stud-screw 6，          6.Bottom and upper rollers 8,      

7. Bottom and upper orbit 2,       8.Magnetic plastic 2,        9.Moving glass(door) 2,   

10. Waterproof 4,               11.Sealant 2,               12. Vertical profile 2,           

13. Wall profile 2   

Ⅳ、Please check the quantity and quality of square parts before install, if you have any inquiry about it please contact our company or dealer without any hesitate, you will get satisfied reply soon!   
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Picture 1

[image: image10.wmf]Ⅴ、Installation Process：
1.   Please put the wall profiles against the wall (Please install it according to the size of glass door), and adjust the profiles perpendicularly by spirit level. Then drill by ф6-8mm driller and put the wall plugs into wall. At last screw down the profile by M5x30 stud screw.(picture 2)
2. Putting the vertical profile in side of fixed glass, inset bottom and upper orbit and screw              down the vertical profile by M4x30 screw (same as another side). Then drill in both of profiles by 3.2dirller.Screw down the decorate cover (picture 3) by M4x12 screw and insert the sealant into vertical profle mall wood board (please make the surface smooth).
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             Picture 2                                Picture 3
3. Installing the bottom and upper rollers on the moving glass door (two glass doors should be same), then inset the waterproof plastic and magnetic plastic on the side glass door and install the handle. Put the moving glass doors into orbits, Pressing the bottom rollers slightly, adjust the height of rollers by wrench until the glass could work well.(picture 4)         
4、 After the installation, all side of glass door should be silicone.  

5、 Please clear the frame by neutral purification after 8 hours.

Ⅵ、Please slide the doors slightly, don’t scratch the frame by strong and sharp material to avoid damaging fittings.
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